                                                                   Revision: 1.0
--------------------------------------------------------------------------------
Package            fix4.2.8-fx.cbsa

Version            4.2.8-fx

Required version   4.2.8

Support models     Server
                   Server Advanced
                   Server 192
                   Virtual Machine

--------------------------------------------------------------------------------
WHAT THIS PACKAGE DOES

 This package fix Evolution system version 4.2.8-p.
 This update is generally done manually by the user following the instructions
 in the INSTALLATION section.

--------------------------------------------------------------------------------
NOTES

 Please clear your browser cache after installing this update.
 
--------------------------------------------------------------------------------
LIMITATIONS

 Nothing.

--------------------------------------------------------------------------------
CHANGES IN THIS RELEASE

[4.2.8-f7]

- Fix: Use yyyy-MM-dd format for SQL date literals


[4.2.8-f6]

- Fix: Remove restrict sqlexec in process point name


[4.2.8-f5]

- Fix: Remove restrict bacnet format in process point name


[4.2.8-f4]

- Fix: Importing ESF duplicates process points if you change the group address
name

[4.2.8-f3]

- Fix: Translator of the annual planner module to Portuguese

[4.2.8-f2]

- Fix: Last ProcessPoint value queue wait for the values, improve performance

[4.2.8-f1]

- Fix: It is not possible to write correctly in the template replacement table.


--------------------------------------------------------------------------------
INSTALLATION

[EVO5 Systems]

  1. Open a web navigator
  2. Enter the address http://<device_IP>/webmin or http://evo5/webmin
  3. Enter the user and password. If the username and password are not known,
     check the product manual or contact with Futurasmus.
  4. In the side menu, navigate to "Others" -> "Custom commands".
  5. Press the button next to "Evolution Package to upload" and search the
     update package file.
  6. Press the "Evolution Package Installer" button. Installation will begin.
     - The installation process can take several minutes. Do not close the
       browser tab or your Evolution system until you have finished.
     - If the system does not have the required previous version installed,
       the installation will be canceled.
     - If the system does not meet the conditions in the LIMITATIONS section,
       the following message will appear and the installation will be canceled.

       ***************************************************
       **                                               **
       **                                               **
       **       YOUR HARDWARE IS NOT COMPATIBLE!        **
       **                                               **
       **                                               **
       ***************************************************

  7. When the installation process is complete, it will display the result.
  8. In the side menu, navigate to "System" -> "Bootup and Shutdown".
  9. At the bottom of the page that opens, press the "Reboot System" button.
 10. Press "Reboot System" button again. The system will restart.

[Other systems]

 1. Open a web navigator
 2. Enter the address http://<device_IP>:8181/upload.php
 3. Enter the user and password. If the username and password are not known,
    check the product manual or contact with Futurasmus.
 4. Press "Select file" button and search the update package file.
 5. Press "INSTALL" button. Installation will begin.
    - The installation process can take several minutes. Do not close the
      browser tab or your Evolution system until you have finished.
    - If the system does not have the required previous version installed,
      the installation will be canceled.
    - If the system does not meet the conditions in the LIMITATIONS section,
      the following message will appear and the installation will be canceled.

      ***************************************************
      **                                               **
      **                                               **
      **       YOUR HARDWARE IS NOT COMPATIBLE!        **
      **                                               **
      **                                               **
      ***************************************************

 6. When the installation process is complete, it will display the result in
    the text field of the web page. After a few seconds the system will
    restart.

